/*###ICF### Section handled by ICF editor, don't touch! ****/
/*-Editor annotation file-*/
/* IcfEditorFile="$TOOLKIT_DIR$\config\ide\IcfEditor\cortex_v1_0.xml" */
/*-Specials-*/
define symbol __ICFEDIT_intvec_start__ = 0x08000000;
/*-Memory Regions-*/
/***** FLASH Part dedicated to M4 *****/
define symbol __ICFEDIT_region_ROM_start__ = 0x08000000;
define symbol __ICFEDIT_region_ROM_end__   = 0x0803FFFF;
define symbol __ICFEDIT_region_RAM_start__ = 0x20000008;
define symbol __ICFEDIT_region_RAM_end__   = 0x20007FFF;
/*-Sizes-*/
define symbol __ICFEDIT_size_cstack__ = 0x1000;
define symbol __ICFEDIT_size_heap__   = 0x400;
/**** End of ICF editor section. ###ICF###*/

define symbol __ICFEDIT_region_RAM_SHARED_start__ = 0x20030000;
define symbol __ICFEDIT_region_RAM_SHARED_end__   = 0x200327FF;

define memory mem with size = 4G;
define region ROM_region        = mem:[from __ICFEDIT_region_ROM_start__   to __ICFEDIT_region_ROM_end__];
define region RAM_region        = mem:[from __ICFEDIT_region_RAM_start__   to __ICFEDIT_region_RAM_end__];
define region RAM_SHARED_region = mem:[from __ICFEDIT_region_RAM_SHARED_start__   to __ICFEDIT_region_RAM_SHARED_end__];

define block CSTACK    with alignment = 8, size = __ICFEDIT_size_cstack__   { };
define block HEAP      with alignment = 8, size = __ICFEDIT_size_heap__     { };

/* MB_MEM1 and MB_MEM2 are sections reserved to mailbox communication. It is placed in the shared memory */
initialize by copy { readwrite };
do not initialize  { section .noinit,
                     section MAPPING_TABLE,
                     section MB_MEM1 };

place at address mem:__ICFEDIT_intvec_start__ { readonly section .intvec };

place in ROM_region        { readonly };
place in RAM_region        { readwrite,block CSTACK, block HEAP };
place in RAM_SHARED_region { first section MAPPING_TABLE};
place in RAM_SHARED_region { section MB_MEM1};
place in RAM_SHARED_region { section MB_MEM2};
